**Section 31 25 14.13 – Hydraulically-Applied Erosion Control:**

**Biotic Erosion Control Matrix**

GENERAL

* 1. SUMMARY

1. This section specifies the Hydraulically-applied Biotic Erosion Control Matrix (BECM) ProGanics® DUAL™. ProGanics DUAL is non-toxic and contains bark and wood fibers that have been phyto-sanitized to eliminate potential weed seeds and pathogens. After phyto-sanitization, a proprietary blend of cross-linked, high-viscosity colloidal polysaccharide biopolymers, biochar, seaweed extract, humic acid, endomycorrhizae, beneficial bacteria and crimped, biodegradable interlocking fibers derived from regenerated plant sources are then added. The resulting ProGanics DUAL formulation will achieve Bonded Fiber Matrix (BFM) erosion control performance while acting to regenerate denuded soils and promote vegetative establishment. Upon application, ProGanics DUAL forms an intimate bond with the soil surface to create a continuous, porous, absorbent and flexible erosion resistant blanket that allows for rapid germination and accelerated plant growth. ProGanics DUAL may require a 12-24 hour curing period to achieve maximum performance.
2. Related Sections: Other Specification Sections, which directly relate to the work of this Section include, but are not limited to the following:
	1. *Section 01 57 00 – Temporary Erosion and Sediment Control*
	2. *Section 02 24 23 – Chemical Sampling and Analysis of Soils*
	3. *Section 31 00 00 – Earthwork*
	4. *Section 31 91 00 – Planting Preparation*
	5. *Section 32 01 90.16 – Amending Soils*
	6. *Section 32 92 00 – Turf and Grasses*

1.02 SUBMITTALS

1. Product Data: Submit manufacturer’s product data and installation instructions. Include required substrate preparation, list of materials and application rate.
2. Certifications: Manufacturer shall submit a letter of certification that the product meets or exceeds all technical and packaging requirements and is made in the U.S.A.

1.03 DELIVERY, STORAGE AND HANDLING

1. Deliver materials and products in UV and weather-resistant factory labeled packages. Store and handle in strict compliance with manufacturer’s instructions and recommendations. Protect from damage, weather, excessive temperatures and construction operations.

PRODUCTS

2.01 ACCEPTABLE MANUFACTURER

1. PROFILE Products LLC

750 Lake Cook Road – Suite 440

Buffalo Grove, IL 60089

International - +1-847-215-1144

United States and Canada – 800-366-1180 (Fax 847-215-0577)

[www.profileproducts.com](http://www.profileproducts.com)

2.02 MATERIALS

1. The BECM shall be ProGanics DUALand conform to the following typical property values when uniformly applied at a rate of 6,500 pounds per acre (7,290 kilograms/hectare) under laboratory conditions.

|  |  |  |  |
| --- | --- | --- | --- |
| **Property** | **Test Method** | **Tested Value (English)** | **Tested Value (SI)** |
| **Physical** |  |  |  |
| Organic Material | ASTM D586 | > 95% | > 95% |
| Mass Per Unit Area | ASTM D65661 | ≥ 21.4 oz/yd2 | ≥ 729 g/m2  |
| Ground Cover | ASTM D65671 | ≥ 99%  | ≥ 99%  |
| Water Holding Capacity | ASTM D7367 | ≥ 850%  | ≥ 850%  |
| pH | ASTM D1293 | 6.0 + 1.0 | 6.0 + 1.0 |
| C:N Ratio | ASTM E1508 & EPA Method 1687 | 50:1 + 10 | 50:1 + 10 |
| Material Color | Observed | Brown | Brown |
| Performance |  |  |  |
| Cover Factor2 | Large Scale Testing4 | ≤ 0.05  | ≤ 0.05  |
| % Effectiveness3 | Large Scale Testing4 | ≥ 95%  | ≥ 95%  |
| Cure time | Observed | 12 - 24 hours | 12 – 24 hours |
| Vegetation Establishment | ASTM D73221 | ≥ 700%  | ≥ 700%  |
| Functional Longevity5 | ASTM D5338 | ≤ 12 months | ≤ 12 months |
| Environmental |  |  |  |
| Ecotoxicity | EPA 2021.0 | 48-hr LC50 > 100% | 48-hr LC50 > 100% |
| Biodegradability | ASTM D5338 | Yes  | Yes |
| EPA 503 Metals – Pass/Fail | EPA 503 Metal Limits6 | Pass | Pass |
| Pathogen Reduction | 40 CFR 503 Class A Compost | Pass | Pass |

1. ASTM test methods developed for Rolled Erosion Control Products and have been modified to accommodate Hydraulically-Applied Erosion Control Products.

2. Cover Factor is calculated as soil loss ratio of treated surface versus an untreated control surface.

3. % Effectiveness = One minus Cover Factor multiplied by 100%.

4. Large scale testing conducted at Utah Water Research Laboratory. For specific testing information please contact a Profile technical servicerepresentative at 800-508-8681 (US and Canada) or +1-847-215-1144 (International).

5. Functional Longevity is the estimated time period, based upon ASTM D5338 testing and field observations, that a material can be anticipated to provide erosion control and agronomic benefits as influenced by composition, as well as site-specific conditions, including; but not limited to – temperature, moisture, light conditions, soils, biological activity, vegetative establishment and other environmental factors.

6. A list of Metals included in the EPA 503 Metal Limits Testing is available upon request.

**2.03 COMPOSITION**

1. All components of the BECM shall be pre-packaged by the manufacturer to assure both material performance and compliance with the following values. Under no circumstances shall field mixing of components be permitted. No chemical additives with the exception of fertilizer, soil neutralizers and biostimulant materials should be added to this product.
	1. Thermally Processed\* Bark and Wood Fibers (within a pressurized vessel) – 85%

\*Heated to a temperature greater than 380 degrees Fahrenheit (193 degrees Celsius) for 5 minutes at a pressure greater than 50 psi (345 kPa)

* 1. Proprietary Blend of cross-linked, high-viscosity colloidal polysaccharide biopolymers, biochar, seaweed extract, humic acid, endomycorrhizae and beneficial bacteria - 11%
	2. Crimped, Biodegradable Interlocking Fibers Derived from Regenerated Plant Sources – 4%
	3. Moisture Content – 12%

**2.04 PACKAGING**

1. Bags: Net Weight – 50 lb (22.7 kg), UV and weather-resistant plastic film

Pallets: Weather-proof, stretch-wrapped with UV resistant pallet cover

Pallet Quantity: 40 bags/pallet or 1 ton (909 kg)/pallet

EXECUTION

3.01 SOIL TESTING

1. Soil Samples shall be taken and sent to a third-party, independent lab for analysis and in compliance with Section 02 24 23 *–* Chemical Sampling and Analysis of Soils, if applicable.
2. The tests shall include analysis and interpretation of results.
3. The soil testing methods used shall be compliant with recognized agronomic testing standards, as outlined in Section 02 24 23, for revegetation of disturbed sites.
4. Soil Analysis shall include results for:
	1. Soil pH
	2. Soluble Salts
	3. Excess Carbonate
	4. Organic Matter
	5. Nutrient readings for:
		1. Nitrogen, Phosphorus, Potassium
		2. Magnesium, Calcium, Sodium, Manganese, Sulfur, Zinc, Copper, Iron, Boron
	6. Cation Exchange Capacity
	7. Percent Base Saturation Sodium
5. BioPrime™, JumpStart™, Aqua-pHix™ and NeutraLime™ Dry or other amendments shall be specified according to Section 32 01 90.16 – Amending Soils and applied with the hydroseeding slurry at Manufacturer recommended rates based on soil test results.

3.02 VEGETATION SPECIES SELECTION

1. Once soils have been analyzed for agronomic potential and amendment recommendations, selection of suitable plant species for achieving sustainable growth and effective erosion control shall be determined by a qualified seed supplier, consulting professional and/or regulatory agency. Species selection and establishment shall be compliant with Section 32 92 00 – Turf and Grasses, if applicable.
2. Site and project specific information considered for species selection shall include:
	1. Project Location and Planning
		1. Climate
		2. Elevation
		3. Aspect
		4. Slope/Gradient
		5. Permanent or Temporary Planting
		6. Installation Date(s)
	2. Soil Conditions
		1. Soil Texture
		2. Soil pH
		3. Toxicities/Deficiencies noted in the previous section.
	3. Site Maintenance Requirements
		1. Mowing
		2. Irrigation
		3. Animal grazing preference
	4. Preferred Vegetation
		1. Drought Tolerant
		2. Native Vegetation
		3. Shrub Species
		4. Turf Grasses
		5. Cool Season
		6. Warm Season
		7. Blend of Cool and Warm Season
		8. Legume Species
		9. Cover Crops

**3.03 SUBSTRATE AND SEEDBED PREPARATION**

1. Examine substrates and conditions where materials will be applied. Apply products to geotechnically stable slopes that have been designed and constructed to divert runoff away from the face of the slope. Do not proceed with installation until satisfactory conditions are established.
2. Depending upon project sequencing and intended application, prepare seedbed in compliance with other specifications under Section 1.01 B

**3.04 INSTALLATION**

1. Strictly comply with equipment manufacturer's installation instructions and recommendations. Use approved hydroseeding machines with fan-type nozzle (50-degree tip). To achieve optimum soil surface coverage, apply BECM from opposing directions to soil surface. Rough surfaces (rocky terrain, cat tracked and ripped soils) may require higher application rates to achieve 100% cover. Slope interruption devices or water diversion techniques are recommended when slope lengths (on a 3H:1V gradient) exceed 50 feet (15 m). Slope interruption intervals may need to be decreased based on steeper slopes or other site conditions. BECM is not recommended for channels or areas with concentrated water flow unless used in conjunction with a rolled erosion control product designed to accommodate the anticipated hydraulic conditions. Unless approved by the Manufacturer, no chemical additives with the exception of fertilizer, soil neutralizers and biostimulant materials should be added to this product.
2. For Erosion Control and Revegetation: To ensure proper application rates, measure and stake area. Due to the higher application rates associated with this product and to achieve maximum performance, apply BECM using a layering process\*:
3. *Apply fertilizer with specified prescriptive agronomic formulations, seed and BECM mixed at a rate of 75 lb per 100 gallons (34 kg / 379 liters) of water over properly prepared surfaces.*

*\*Layering of BECM is typically necessary to achieve higher application rates and more uniform coverage. Confirm loading rates with equipment manufacturer.*

 *Best results and more rapid curing are achieved at temperatures exceeding 60°F (15°C). Curing times may be accelerated in high temperature, low humidity conditions with product applied on dry soils. Do not apply if precipitation is imminent within 24-48 hours.*

1. Mixing: A mechanically agitated hydroseeding machine is strongly recommended:
2. *Fill 1/3 of mechanically agitated hydroseeder with water. Turn pump on for 15 seconds and purge and pre-wet lines. Turn pump off.*
3. *Turn agitator on and load low density materials first (i.e. seed).*
4. *Continue slowly filling tank with water while loading fiber matrix into tank.*
5. *Consult application and loading charts to determine number of bags to be added for desired area and application rate.* *Mix at a rate of 75 lb of BECM per 100 gallons of water (34 kg/379 liters). Contact Equipment manufacturer to confirm optimum mixing rates.*
6. *All BECM should be completely loaded before water level reaches 3/4 of tank capacity.*
7. *Add fertilizer and any other remaining amendments when tank is approximately 3/4 full.*
8. *Top off with water and mix until all fiber is fully broken apart and hydrated (minimum of 10 minutes — increase mixing time when applying in cold conditions). This is very important to fully activate the bonding additives and to obtain proper viscosity.*
9. *Shut off recirculation valve to minimize potential for air entrainment within the slurry.*
10. *Slow down agitator and start applying with a 50-degree fan tip nozzle.*
11. *Spray in opposing directions for maximum soil coverage.*
12. Application Rates: These application rates are for standard conditions on rough graded slopes. Designers and applicators may wish to increase application rates on cat tracked and extremely rough surfaces. If both Soil Organic Matter and Slope Gradient information are available, apply the higher rate of material per the two selection parameters.

|  |  |  |  |
| --- | --- | --- | --- |
| **% Soil Organic Matter** | **Slope Gradient / Condition** | **English (lb/ac)** | **Metric (kg/ha)** |
| < 5.0 and ≥ 1.5 | ≤ 4H to 1V | 4,000 lb/ac | 4,480 kg/ha |
| < 1.5 and ≥ 0.75 | > 4H to 1V and ≤ 3H to 1V | 5,500 lb/ac | 6,160 kg/ha |
| < 0.75 | > 3H to 1V and ≤ 2H to 1V | 6,500 lb/ac | 7,290 kg/ha |

For additional details including mixing ratios/loading rates for specific machine sizes and visual keys for proper application, please consult Profile® Application Guide BECM.

3.05 CLEANING AND PROTECTION

1. Always flush residual slurry from hydraulic seeding/mulching equipment immediately following each application, at the end of each work period or when equipment will be left unattended. Compounds containing residual Urea, Nitrogen, Phosphorus, Potassium and other substances may form and can be hazardous to human health and equipment.
2. Clean spills promptly. Advise owner of methods for protection of treated areas. Do not allow treated areas to be trafficked or subjected to grazing.

3.06 INSPECTION AND MAINTENANCE

1. All inspections and maintenance recommendations shall be conducted by qualified professionals consistent with the owner, engineer/specifier and regulatory entity(ies) expectations.
2. Initial inspections shall insure installations are in accordance with the project plans and specifications with material quantities and activities fully documented. Refer to Section 32 92 00 – Turf and Grasses for any additional details.
3. Subsequent inspections shall be conducted at pre-determined time intervals and corrective maintenance activities directed after each significant precipitation or other potentially damaging weather or site event.

**D ENGLISH SI**

© 2019 PROFILE Products LLC. All Rights Reserved. A copyright license to reproduce this specification is hereby granted to non-manufacturing landscape architects, specification writers and designers.

Revision Date: 08/2019